SIMISA@@@@@@@@@@JINX0D0t______
 
 Wagon ( 122022 
  Type ( Engine ) 
  WagonShape ( 122022.s ) 
 
 Comment ( Eng created by ZSR - http://csd.webzdarma.cz ) 
 Comment ( Datum: 14/12/2010 ) 
 Comment ( Version: 1.06 ) 
 Comment ( Model: Pikku 2013 ) 
 Comment ( Svetla: reflektor 2 zarovky pouze dalkovy ) 
 Comment ( Ostatni: sd modifikovan na 30cm ) 
 Comment ( Eng obsahuje ovladani dvou sberacu ) 
 Comment ( Uprava 2 ) 
 Comment ( Oprava eng+cvf = bob57_cz - 2010-12-24 ) 
 
 comment ( Overall physics ) 
  Size ( 3.15m 4.72m 17.00m ) 
  CentreOfGravity ( 0m 1.9m 0m ) 
  Mass ( 85t ) 
  WheelRadius ( 0.625m ) 
  InertiaTensor ( Box ( 3.15m 4.72m 17.00m ) ) 
 
 comment	( Coupling ) 
 comment ( Rear Coupler ) 
  Coupling ( 
   Type ( Chain ) 
   Spring ( 
    Stiffness ( 7.5e6N/m 1e7N/m ) 
    Damping ( 1e6N/m/s 2e6N/m/s ) 
    Break ( 1.1e8N 5e8N ) 
    r0 ( 30cm 60cm ) 
    ) 
  CouplingHasRigidConnection ( 0 ) 
  Velocity ( 0.01m/s ) 
    ) 
 
 Buffers ( 
  Spring ( 
  Stiffness ( 1e6N/m 5e6N/m ) 
  Damping ( 1e6N/m/s 1e6N/m/s ) 
  r0 ( 6cm 30cm ) 
    ) 
    Centre ( 0.5 ) 
    Radius ( 1 ) 
    Angle ( 0.5deg ) 
    ) 
 
 comment ( Adhesion and Friction ) 
  Adheasion ( 0.4 0.8 1.15 0 ) 
  DerailRailHeight ( 10cm ) 
  DerailRailForce ( 2.5*85t ) 
  DerailBufferForce ( 800kN ) 
  NumWheels ( 4 ) 
  PassengerCapacity ( 10 ) 
  Friction ( 4000N/m/s  0  1mph  12N/m/s  2.15  5.1N/rad/s  1  -1rad/s  0  1 ) 
 
 comment ( Wagon Brakes ) 
 Comment ( P=44kN, G=30kN ) 
  MaxBrakeForce ( 44kN ) 
  MaxHandbrakeForce ( 16kN ) 
  NumberOfHandbrakeLeverSteps ( 100 ) 
 
 Comment ( nastaven bezpecnejsi brzdovy rezim P ) 
 Comment ( Predpis CD V15/I pl. od 1.1.2002 cl. 39: Ve vlaku brzdenem v rezimu G muze byt lokomotiva ovladajici brzdu v rezimu P a pri Lv jizde dokonce MUSI ) 
 
  BrakeEquipmentType ( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" ) 
  BrakeSystemType ( "Air_single_pipe" ) 
  TripleValveRatio ( 2.53 ) 
  MaxReleaseRate ( 1.01 ) 
  MaxApplicationRate ( 1.4 ) 
  MaxAuxilaryChargingRate ( 2.4 ) 
  BrakeCylinderPressureForMaxBrakeBrakeForce ( 56 ) 
  EmergencyResVolumeMultiplier ( 1 ) 
  EmergencyResCapacity ( 1.88 ) 
  EmergencyResChargingRate ( 3 ) 
  EmergencyBrakeResMaxPressure ( 73 ) 
 
 comment ( Freight, Inside, IntakePoint ) 
  Inside ( 
   PassengerCabinFile ( 122022.s ) 
   PassengerCabinHeadPos ( -1.7 3.0 6.62 ) 
   RotationLimit ( 100 180 0 ) 
   StartDirection ( 0 -90 0 ) 
    ) 
 
 comment ( Lights ) 
 
  Lights ( 29 
 
 comment ( definice svetelnych kuzelu ) 

		Light ( comment ( kuzelove svetlo obrysove )
			Type ( 1 ) 
			Conditions ( 
				Headlight ( 1 ) 
				Unit ( 0 ) 
				Coupling ( 0 ) 
				Control ( 2 ) 
				Service ( 2 ) 
				TimeOfDay ( 2 ) 
			) 
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 33333333 ) 
					Position ( 0.0 2.0 2.0 ) 
					Angle ( 25 ) 
					Transition ( 0 ) 
					Radius ( 25 ) 
				)
			)
		)
		Light ( comment ( kuzelove svetlo tlumene )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 44444444 )
					Position ( 0 3.5 2.0 )
					Angle ( 15 )
					Transition ( 0 )
					Radius ( 350 )
				)
			)
		)
		Light ( comment ( kuzelove svetlo dalkove )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 88888888 )
					Position ( 0 3.5 2.0 )
					Angle ( 15 )
					Transition ( 0 )
					Radius ( 350 )
				)
			)
		)

 comment ( definice svetel pro obe stanoviste )

		Light ( comment ( predni bile leve off ) 
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 1 ) 
				Unit ( 0 ) 
				Coupling ( 0 ) 
				Control ( 0 ) 
				Service ( 2 ) 
			) 
			FadeIn ( 0.1 ) 
			FadeOut ( 0.1 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0 ) 
					LightColour ( FFEED15D ) 
					Position ( -0.805 1.915 8.07 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.6 ) 
				) 
			) 
		) 
		Light ( comment ( predni bile prave off )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Coupling ( 0 ) 
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni bile leve off )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Coupling ( 0 ) 
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni bile prave off )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 0 )
				Coupling ( 0 ) 
				Control ( 0 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
 
 comment ( definice svetel pro predni stanoviste )

		Light ( comment ( predni reflektor tlumeneL )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.08 3.68 7.99 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light ( comment ( predni reflektor tlumeneR )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.08 3.68 7.98 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light ( comment ( predni reflektor plneL )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.08 3.68 7.99 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light ( comment ( predni reflektor plneR )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.08 3.68 7.96 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light ( comment ( predni bile leve zapnuto )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( predni bile prave zapnuto )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni cervene leve )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AFFF0000 )
					Position ( -0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni cervene prave )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AFFF0000 )
					Position ( 0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)

 comment ( definice svetel pro zadni stanoviste )

		Light ( comment ( predni reflektor tlumeneL )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.08 3.68 -7.97 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( predni reflektor tlumeneR )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.08 3.68 -7.97 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( predni reflektor plneL )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.08 3.68 -7.97  )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( predni reflektor plneR )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.08 3.68 -7.97  )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( predni bile leve zapnuto )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( predni bile prave zapnuto )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni cervene prave )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AFFF0000 )
					Position ( -0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( zadni cervene leve )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AFFF0000 )
					Position ( 0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)

 comment ( Definice svetel pro loko ovladanou PC )

		Light ( comment ( PC reflektor predniL )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.08 3.68 7.97 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( PC reflektor predniR )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.08 3.68 7.97 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.2 )
				)
			)
		)
		Light ( comment ( PC predni prave )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( 0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( PC predni leve )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFEED15D )
					Position ( -0.805 1.915 8.07 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( PC zadni leve )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light ( comment ( PC zadni prave )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.805 1.915 -8.07 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
	)
 
 comment ( EngSound ) 
  Sound ( "..//..//common.snd//sndelok//122eng.sms" ) 
 ) 
 
 Engine ( 122022 
 
 comment ( Description ) 
  Wagon ( 122022 ) 
   
 comment ( Basic physical engine data ) 
  Type ( Electric ) 
  MaxPower ( 2188kW ) 
  MaxForce ( 1903kN ) 
  MaxContinuousForce ( 1903kN ) 
  MaxCurrent ( 5450A ) 
  MaxVelocity ( 90km/h ) 
  DieselEngineSpeedOfMaxTractiveEffort ( 0mph ) 
  WheelRadius ( 0.625m ) 
 
 comment ( sanding system is switched off when faster than given velocity ) 
  Sanding ( 1e9mph ) 
  NumWheels ( 4 ) 
 
 comment ( CabSound and Views ) 
  Sound ( "..//..//common.snd//sndelok//122cab.sms" ) 
  CabView ( "122.cvf" ) 
  HeadOut ( 1.7 3.0 6.62 ) 
 
 comment ( Brakes ) 
  AirBrakesAirCompressorPowerRating ( 1.09 ) 
  AirBrakesMainMinResAirPressure ( 56 ) 
  AirBrakesMainMaxAirPressure ( 116 ) 
  AirBrakesMainResVolume ( 36 ) 
  AirBrakesAirCompressorWattage ( 32000 ) 
  AirBrakesCompressorRestartPressure ( 87 ) 
  AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 ) 
  AirBrakesHasLowPressureTest ( 1 ) 
  AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
  
  EngineBrakesControllerHasProportionalBrake ( 1 ) 
  EngineBrakesControllerMaxApplicationRate ( 5 ) 
  EngineBrakesControllerMaxReleaseRate ( 5 ) 
  EngineBrakesControllerEmergencyApplicationRate ( 10 ) 
  EngineBrakesControllerMinSystemPressure ( 0 ) 
  EngineBrakesControllerMaxSystemPressure ( 73 ) 
  EngineBrakesControllerFullServicePressureDrop ( 73 ) 
  EngineBrakesControllerDirectControlExponent ( 1 ) 
  EngineBrakesProportionalBrakeLag ( 0.8 ) 
 
  TrainBrakesControllerMinPressureReduction ( 1 ) 
  TrainBrakesControllerMaxApplicationRate ( 1.7 ) 
  TrainBrakesControllerMaxReleaseRate ( 1.1 ) 
  TrainBrakesControllerMaxQuickReleaseRate ( 1.5 ) 
  TrainBrakesControllerEmergencyApplicationRate ( 4.7 ) 
  TrainBrakesControllerMinSystemPressure ( 3 ) 
  TrainBrakesControllerMaxSystemPressure ( 73 ) 
  TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
  TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 ) 
  TrainPipeLeakRate ( 0.02 ) 
  TrainBrakesControllerFullServicePressureDrop ( 22 ) 
 
  BrakesEngineBrakeType ( "Air_single_pipe"  ) 
  BrakesTrainBrakeType ( "Air_single_pipe" ) 
  BrakesEngineControllers ( "Independent, Train" ) 
 
  DoesBrakeCutPower ( 1 ) 

 comment ( Monitors ) 
 
  OverspeedMonitor ( 
   MonitoringDeviceMonitorTimeLimit ( 0 ) 
   MonitoringDeviceAlarmTimeLimit ( 5 ) 
   MonitoringDevicePenaltyTimeLimit ( 0 ) 
   MonitoringDeviceResetLevel ( 0 ) 
   MonitoringDeviceTriggerOnHighCurrent ( 750 ) 
   MonitoringDeviceAppliesFullBrake ( 0 ) 
   MonitoringDeviceAppliesEmergencyBrake ( 0 ) 
   MonitoringDeviceAppliesCutsPower ( 0 ) 
   MonitoringDeviceAppliesShutsDownEngine ( 1 ) 
   MonitoringDeviceDoesSuppressionReset ( 0 ) 
   MonitoringDeviceResetOnZeroSpeed ( 0 ) 
   MonitoringDeviceResetOnDirectionNeutral ( 1 ) 
   MonitoringDeviceResetOnResetButton ( 0 ) 
   ) 
 
  VigilanceMonitor ( 
   MonitoringDeviceMonitorTimeLimit ( 27 ) 
   MonitoringDeviceAlarmTimeLimit ( 17 ) 
   MonitoringDevicePenaltyTimeLimit ( 0 ) 
 Comment ( MonitoringDeviceCriticalLevel ( 55.9 ) ) 
   MonitoringDeviceResetLevel ( 0 ) 
   MonitoringDeviceAppliesFullBrake ( 0 ) 
   MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
   MonitoringDeviceAppliesCutsPower ( 1 ) 
   MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
   MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) 
 Comment ( MonitoringDeviceTriggerOnOverspeed ( 56 ) ) 
 Comment ( MonitoringDeviceTriggerOnTrackOverspeed ( 1 ) ) 
 Comment ( MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 ) ) 
   MonitoringDeviceResetOnZeroSpeed ( 1 ) 
   MonitoringDeviceResetOnResetButton ( 1 ) 
   ) 
 
  EmergencyStopMonitor ( 
   MonitoringDeviceMonitorTimeLimit ( 0 ) 
   MonitoringDeviceAlarmTimeLimit ( 0 ) 
   MonitoringDevicePenaltyTimeLimit ( 0 ) 
   MonitoringDeviceCriticalLevel ( 0 ) 
   MonitoringDeviceResetLevel ( 0 ) 
   MonitoringDeviceAppliesFullBrake ( 1 ) 
   MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
   MonitoringDeviceAppliesCutsPower ( 1 ) 
   MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
   MonitoringDeviceResetOnZeroSpeed ( 1 ) 
   ) 
 
 comment ( Controllers ) 
 
 EngineControllers ( 
 
  Throttle ( 0 1 0.005 0 
  NumNotches ( 48
  Notch ( 0.0   0 Dummy )
  Notch ( 0.001 0 Dummy )
  Notch ( 0.02  0 Dummy )
  Notch ( 0.04  0 Dummy )
  Notch ( 0.06  0 Dummy )
  Notch ( 0.08  0 Dummy )
  Notch ( 0.10  0 Dummy )
  Notch ( 0.12  0 Dummy )
  Notch ( 0.13  0 Dummy )
  Notch ( 0.14  0 Dummy )
  Notch ( 0.15  0 Dummy )
  Notch ( 0.16  0 Dummy )
  Notch ( 0.17  0 Dummy )
  Notch ( 0.18  0 Dummy )
  Notch ( 0.19  0 Dummy )
  Notch ( 0.20  0 Dummy )
  Notch ( 0.21  0 Dummy )
  Notch ( 0.22  0 Dummy )
  Notch ( 0.23  0 Dummy )
  Notch ( 0.24  0 Dummy )
  Notch ( 0.25  0 Dummy )
  Notch ( 0.26  0 Dummy )
  Notch ( 0.27  0 Dummy )
  Notch ( 0.28  0 Dummy )
  Notch ( 0.29  0 Dummy )
  Notch ( 0.30  0 Dummy )
  Notch ( 0.31  0 Dummy )
  Notch ( 0.33  0 Dummy )
  Notch ( 0.35  0 Dummy )
  Notch ( 0.37  0 Dummy )
  Notch ( 0.375 0 Dummy )
  Notch ( 0.38  0 Dummy )
  Notch ( 0.385 0 Dummy )	
  Notch ( 0.39  0 Dummy )
  Notch ( 0.395 0 Dummy )
  Notch ( 0.40  0 Dummy )
  Notch ( 0.41  0 Dummy )
  Notch ( 0.45  0 Dummy )
  Notch ( 0.49  0 Dummy )
  Notch ( 0.53  0 Dummy )
  Notch ( 0.57  0 Dummy )
  Notch ( 0.61  0 Dummy )
  Notch ( 0.65  0 Dummy )
  Notch ( 0.72  0 Dummy )
  Notch ( 0.79  0 Dummy )
  Notch ( 0.86  0 Dummy )
  Notch ( 0.93  0 Dummy )
  Notch ( 1.00  0 Dummy )
  ) ) 
 
 comment ( ***Primocinna brzda typ DAKO-BP*** ) 
  Brake_Engine ( 0 0.76 0.05 0 
  NumNotches ( 1 
  Notch ( 0 1 Dummy ) 
  ) ) 
 
 comment ( ***Prubezna brzda typ DAKO-BS2*** ) 
  Brake_Train ( 0 1 0.04 0.21 
  NumNotches ( 7 
  Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart ) 
  Notch ( 0.14 0 TrainBrakesControllerReleaseStart ) 
  Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart ) 
  Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart ) 
  Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
  Notch ( 0.87 0 TrainBrakesControllerSuppressionStart ) 
  Notch ( 0.99 0 TrainBrakesControllerEmergencyStart ) 
  ) ) 
 
  Brake_Hand ( 0 1 0.0125 0 
  NumNotches ( 0 ) 
  ) 
 
 DirControl ( -1 0 1 1 ) 
 BellToggle ( 0 1 0 ) 
 AWS ( 0 1 0 ) 
 Sanding ( 0 1 0 ) 
 Horn ( 0 1 0 ) 
 Wipers ( 0 1 0 ) 
 EmergencyStopToggle ( 0 1 0 ) 
 Vigilance ( 0 1 0 ) 
 PantographToggle1 ( 0 1 0 ) 
 PantographToggle2 ( 0 1 0 ) 
 PantographsToggle_4 ( 0 1 0 ) 
 Headlights ( 0 0.25 1 0 ) 
 BailOffButton ( 0 1 0 ) 
  ) 

Name ( "CDC 122 022-7" )

 Comment ( Operations ) 
 Description (
 "Ovladani\n\n"+ 
 "Lokomotiva ma oba sberace ovladatelne pomoci 4-polohoveho prepinace bez koncove polohy, ovlada se standardne klavesou P\n\n"+ 
 "Vykon 31% odpovida 25. hospodarnemu seriovemu stupni\n\n"+ 
 "Vykon 65% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
 "Po 25. hospodarnem stupni nasleduji 3 stupne shuntovaci a pak se kontroler vraci zpet postupne na hospodarny stupen\n\n"+
 "Rozjezdove stupne muzete zatezovat pouze po dobu 6s, proto lokomotivy vzdy prevedte na hospodarne nebo shuntovaci stupne co nejrychleji\n\n"+ 
 "Pretizeni:\n"+
 "Proud trvaly : 365A\n\n"+
 "60min: 420A\n\n"+
 "Nadproudova ochrana : 750A\n\n"+ 
 "Brzdic prubezne vlakove brzdy DAKO BS2\n\n"+
 "Brzdic lokomotivni brzdy DAKO-BP\n\n"+	
 "Rada CD 122 je elektricka skrinova lokomotiva, pouzivana prevazne v nakladni doprave.\n\n"+
 "Typ Bo'-Bo', napeti 3 kV ss.\n\n"+
 "Delka pres narazniky: 17,21 m\n\n"+
 "Prumer hnacich kol: 1250 mm\n\n"+
 "Hmotnost ve sluzbe: 85 t\n\n"+
 "Trvaly vykon trakcnich motoru: 2040 kW\n\n"+
 "Max. rychlost 90 km/h\n\n"+
 "Trvaly proud trakcnich motoru: 365 A\n\n"+
 "Hodinovy proud trakcnich motoru: 420 A\n\n"+
 "Trvala tazna sila : 147 kN\n\n"+
 "Hodinova tazna sila : 179 kN\n\n"
 ) 
 
 EngineOperatingProcedures ( 
 "Stupne kontroleru:\n"+
 "1.-24.	 Rozjezdove stupne seriove\n"+
 "25. 31% Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
 "I.-III. Shuntovaci stupne, vsechny motory v serii\n"+
 "26.-35. Odporove serioparalelni stupne (vzdy dva motory v serii)\n"+
 "36. 65% Hospodarny serioparalelni stupen (odporniky vyrazeny)\n"+
 "I.-V.	 Shuntovaci stupen pro serioparalelni zapojeni motoru\n\n"
 ) 
 ) 
 