SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd141_004
	Type ( Engine )
	WagonShape ( cd141_004.s )

	Comment ( model Pikku, nastaveni pro msts-bin 1.6 bob57_cz-2006-12-06a )

	Comment ( Eng modified by ZSR - http://csd.webzdarma.cz )
	Comment ( Version 1.1 release )
	Comment ( Datum: 22.01.2008 - Tygy - nastaveni svetel pro predpis CD )
	Comment ( Vyladena kompletni vykonova charakteristika - adheasion, friction, maxpower, maxcurrent, maxforce )
	Comment ( Umisten brzdic Skoda N/O - dle originalni dokumentace )
	Comment ( Uprava v brzdach )

	Size ( 3.147m 4.585m 15.8m )
	Mass ( 84.0t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box (3.147m 4.585m 15.8m) )

	Coupling ( 
		Type ( Chain ) 
			Spring ( 
			Stiffness ( 7.5E6N/m 1E7N/m ) 
			Damping ( 1E6N/m/s 2E6N/m/s ) 
			Break ( 1.1E7N 5E7N ) 
			r0 ( 30cm 60cm ) 
		) 
		CouplingHasRigidConnection ( 0 ) 
		Velocity ( 0.01m/s ) 
	) 
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 10cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.114 0.64 1.35 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*84t )
	DerailBufferForce ( 350kN )
	NumWheels (	4 )
	Friction (
		1051.4N/m/s		-0.1		1.3mph		14.200N/m/s		2.100
		5.1N/rad/s		1		-1rad/s		0		1
	)

comment	( Brzdy vozu )

	MaxBrakeForce( 51kN )
	MaxHandbrakeForce( 26kN )
	NumberOfHandbrakeLeverSteps( 100 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 1.1 )
	MaxApplicationRate( 1.1 )
	MaxAuxilaryChargingRate( 3 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 55 )
        EmergencyResVolumeMultiplier ( 11 )
        EmergencyResCapacity( 0.88 )
	EmergencyResChargingRate( 1 )
	EmergencyBrakeResMaxPressure( 73 )  
	
	Lights	( 23

	comment ( Nastaveni svetel hrace )

	Light (		comment ( 1 predni bile leve )
	Type 		( 0 )
	Conditions 	(
	Headlight	( 1 )
	Unit 		( 0 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( -0.87 1.50 7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 3 predni bile prave )
	Type 		( 0 )
	Conditions 	(
	Headlight	( 1 )
	Unit 		( 0 )
				)
	FadeIn		( 0.1 )
	FadeOut 	( 0.3 )
	Cycle		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.87 1.50 7.5 )
	Azimuth		( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 1_1 predni bile leve )
	Type 		( 0 )
	Conditions 	(
	Headlight	( 4 )
	Unit 		( 2 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( -0.87 1.50 7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 3_1 predni bile prave )
	Type 		( 0 )
	Conditions 	(
	Headlight	( 4 )
	Unit 		( 2 )
				)
	FadeIn		( 0.1 )
	FadeOut 	( 0.3 )
	Cycle		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.87 1.50 7.5 )
	Azimuth		( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 2 predni cervene leve )
	Type		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 4 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( -0.87 1.50 7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)

	Light (		comment ( 4 predni cervene prave )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 4 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( 0.87 1.50 7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)

	Light (		comment ( 5 zadni bile leve )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 1 )
	Unit 		( 0 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( -0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 7 zadni bile prave )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 1 )
	Unit 		( 0 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 5_1 zadni bile leve )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 5 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( -0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 7_1 zadni bile prave )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 5 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( 6 zadni cervene leve )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 3 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( -0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)

	Light (		comment ( 8 zadni cervene prave )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 4 )
	Unit 		( 3 )
				)
	FadeIn 		( 0.1 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( 0.87 1.50 -7.5 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)

	Light (		comment ( 9 kuzelove svetlo tlumene )
	Type 		( 1 )
	Conditions 	(
	Headlight 	( 2 )
	Unit 		( 2 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( FF808080 )
	Position 	( 0 3.5 4 )
	Angle 		( 25 )
	Transition 	( 0 )
	Radius 		( 80 )
	)	)	)

	Light (		comment ( 10 kuzelove svetlo dalkove )
	Type 		( 1 )
	Conditions 	(
	Headlight 	( 3 )
	Unit 		( 2 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.2 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( FFFFFFFF )
	Position 	( 0 3.5 4 )
	Angle 		( 15 )
	Transition 	( 0 )
	Radius 		( 400 )
	)	)	)

	Light (		comment ( 11 predni reflektor tlumene )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 2 )
	Unit 		( 2 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.5 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.0 3.60 7.42 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.4 )
	)	)	)

	Light (		comment ( 13 predni reflektor plne )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 3 )
	Unit 		( 2 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.5 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( ffF5F480 )
	Position 	( 0.0 3.60 7.42 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.9 )
	)	)	)

	Light (		comment ( 15 zadni reflektor tlumene )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 2 )
	Unit 		( 5 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.5 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.0 3.60 -7.42 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.4 )
	)	)	)

	Light (		comment ( 17 zadni reflektor plne )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 3 )
	Unit 		( 5 )
				)
	FadeIn 		( 0.2 )
	FadeOut 	( 0.5 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( ffF5F480 )
	Position 	( 0.0 3.60 -7.42 )
	Azimuth 	( 180 180 180 )
	Transition 	( 0 )
	Radius 		( 0.9 )
	)	)	)

	comment ( TRF loco rizena PC  )

	Light (		comment ( TRF11 predni reflektor tlumene )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 0 )
	Unit 		( 5 )
	Service 	( 2 )
	Control 	( 1 )
				)
	FadeIn 		( 1.0 )
	FadeOut 	( 1.0 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 60EED15D )
	Position 	( 0.0 3.60 -7.42 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.4 )
	)	)	)

	Light	(		comment( TRF1 predni bile leve )
	Type		( 0 )
	Conditions	(
	Headlight 	( 0 )
	Unit 		( 2 )
	Service 	( 2 )
	Control 	( 1 )
				)
	FadeIn		( 1.0 )
	FadeOut		( 1.0 )
	Cycle		( 0 )
	States	( 1
	State	(
	Duration 	( 0.0 )
	LightColour ( 60EED15D )
	Position 	( -0.87 1.50 7.5 )
	Azimuth 	( 0.0 0.0 0.0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light	(		comment( TRF3 predni bile prave )
	Type		( 0 )
	Conditions	(
	Headlight 	( 0 )
	Unit 		( 2 )
	Service 	( 2 )
	Control 	( 1 )
				)
	FadeIn		( 1.0 )
	FadeOut		( 1.0 )
	Cycle		( 0 )
	States	(	1
	State	(
	Duration 	( 0.0 )
	LightColour ( 60EED15D )
	Position 	( 0.87 1.50 7.5 )
	Azimuth 	( 0.0 0.0 0.0 )
	Transition 	( 0 )
	Radius 		( 0.7 )
	)	)	)

	Light (		comment ( TRF11 zadni cervene leve )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 0 )
	Unit 		( 2 )
	Service 	( 2 )
	Control 	( 1 )
				)
	FadeIn 		( 1.0 )
	FadeOut 	( 1.0 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( -0.87 1.50 -7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)

	Light (		comment ( TRF12 zadni cervene prave )
	Type 		( 0 )
	Conditions 	(
	Headlight 	( 0 )
	Unit 		( 2 )
	Service 	( 2 )
	Control 	( 1 )
				)
	FadeIn 		( 1.0 )
	FadeOut 	( 1.0 )
	Cycle 		( 0 )
	States ( 1
	State (
	Duration 	( 0 )
	LightColour ( 80ff0000 )
	Position 	( 0.87 1.50 -7.5 )
	Azimuth 	( 0 0 0 )
	Transition 	( 0 )
	Radius 		( 0.5 )
	)	)	)
	)

comment	( EngSound, Freight, Inside )
	Comment ( ../../common.snd/Cd_Elok_v1/141eng.sms )
	Comment ( "../../common.snd/Cd_Elok_v2/140eng.sms" )
	Sound ( "../../common.snd/sndelok/141eng.sms" )
	Comment ( "141eng.sms" )
)

Engine ( cd141_004

	Wagon	( cd141_004 )
	Name	( " CD 141.004-2" )

	Type ( Electric )
	MaxVelocity								( 132km/h )
	MaxPower								( 2814kW )
	MaxForce								( 1248kN )	
	MaxContinuousForce						( 1248kN )
	MaxCurrent								( 4581A )
	DieselEngineSpeedOfMaxTractiveEffort	( 0mph )
	WheelRadius								( 0.625m )
	NumWheels								( 4 )
	Sanding									( 60km/h )
	MaxSandingTime                         	( 600 )
	DoesBrakeCutPower                      	( 1 )
	DoesHornTriggerBell                    	( 0 )
	
comment	( CabSound and Views )
	Comment ( ../../common.snd/Cd_Elok_v2/141cab.sms )
	Comment ( "../../common.snd/Cd_Elok_v2/140cab.sms" )
	Sound   ( "../../common.snd/sndelok/141cab.sms" )
	Comment ( "141cab.sms" )

	Comment ( ../../common.cab/Cd_140_v1/cab140.cvf )
	Comment ( ../../common.cab/Cd_140_v2/140.cvf )
	Comment ( "../../common.cab/cab140/140.cvf" )
	Comment ( CabView ( "cd_121.cvf" ) )

	CabView ( "../../common.cab/cab141/141.cvf" )
	Comment ( "../../common.cab/cab141/cd141.cvf" )	
	
	HeadOut ( 1.6 2.9 6.2 ) 	
	

comment	( Brzdy loko )

	BrakesEngineBrakeType	( Air_single_pipe )
	BrakesTrainBrakeType	( Air_single_pipe )
	BrakesEngineControllers	( "Hand, Train, Independent" )

	AirBrakesAirCompressorPowerRating ( 1.18 )
	AirBrakesMainMinResAirPressure ( 56 )
	AirBrakesMainMaxAirPressure ( 102 )	
	AirBrakesMainResVolume ( 32.84 )
	AirBrakesAirCompressorWattage ( 15000 )
	AirBrakesCompressorRestartPressure ( 80 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 )
	AirBrakesHasLowPressureTest ( 1 )
	AirBrakesIsCompressorElectricOrMechanical ( 0 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerFullServicePressureDrop ( 21 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 3 )
	TrainBrakesControllerMaxApplicationRate ( 1.3 )
	TrainBrakesControllerMaxReleaseRate ( 1.5 )
	TrainBrakesControllerMaxQuickReleaseRate ( 2.5 )
	TrainBrakesControllerEmergencyApplicationRate ( 5 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 60 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22 )
	TrainPipeLeakRate ( 0.033 )
	TrainBrakesControllerFullServicePressureDrop ( 22 )

comment	( Monitors )

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 80 )
		MonitoringDeviceAlarmTimeLimit( 40 )
		MonitoringDevicePenaltyTimeLimit ( 90 ) 
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceTriggerOnOverspeed ( 77.6 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 ) 
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 ) 
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)
		
	OverSpeedMonitor(
		MonitoringDeviceTriggerOnHighCurrent ( 700A )
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnDirectionNeutral( 1 )
		)

Comment ( End of Monitors )
		
comment	( Controllers )

	EngineControllers (

		AWS					( 0 1 0 )
		BailOffButton		( 0 1 0 )
		BellToggle			( 0 1 0 )
		DirControl			( -1 0 1 1 )
		EmergencyStopToggle	( 0 1 0 )
		Headlights			( 0 0.25 1 0 )
		Horn				( 0 1 0 )

		PantographToggle1 	( 0 1 0 ) 
		PantographToggle2		( 0 1 0 ) 
		PantographsToggle_5 	( 0 1 2 ) 

		Sanding				( 0 1 0 )
		Vigilance			( 0 1 0 )
		Wipers				( 0 1 0 )

	Throttle ( 0 1 0.005 0
	NumNotches ( 48
	Notch ( 0.0   0 Dummy )
	Notch ( 0.004 0 Dummy )

	Notch ( 0.02  0 Dummy )
	Notch ( 0.03  0 Dummy )
	Notch ( 0.05  0 Dummy )
	Notch ( 0.06  0 Dummy )
	Notch ( 0.08  0 Dummy )

	Notch ( 0.10  0 Dummy )
	Notch ( 0.12  0 Dummy )
	Notch ( 0.13  0 Dummy )
	Notch ( 0.14  0 Dummy )
	Notch ( 0.15  0 Dummy )

	Notch ( 0.16  0 Dummy )
	Notch ( 0.18  0 Dummy )
	Notch ( 0.20  0 Dummy )
	Notch ( 0.22  0 Dummy )
	Notch ( 0.24  0 Dummy )

	Notch ( 0.26  0 Dummy )
	Notch ( 0.28  0 Dummy )
	Notch ( 0.30  0 Dummy )
	Notch ( 0.32  0 Dummy )
	Notch ( 0.34  0 Dummy )

	Notch ( 0.35  0 Dummy )
	Notch ( 0.36  0 Dummy )
	Notch ( 0.37  0 Dummy )

	Notch ( 0.38  0 Dummy )

	Notch ( 0.41  0 Dummy )
	Notch ( 0.44  0 Dummy )
	Notch ( 0.47  0 Dummy )
	Notch ( 0.50  0 Dummy )

	Notch ( 0.505 0 Dummy )
	Notch ( 0.510 0 Dummy )
	Notch ( 0.515  0 Dummy )

	Notch ( 0.52  0 Dummy )
	Notch ( 0.53  0 Dummy )
	Notch ( 0.55  0 Dummy )
	Notch ( 0.57  0 Dummy )
	Notch ( 0.59  0 Dummy )
	Notch ( 0.61  0 Dummy )
	Notch ( 0.62  0 Dummy )
	Notch ( 0.63  0 Dummy )

	Notch ( 0.64  0 Dummy )

	Notch ( 0.71  0 Dummy )
	Notch ( 0.78  0 Dummy )
	Notch ( 0.85  0 Dummy )
	Notch ( 0.93  0 Dummy )
	Notch ( 0.999 0 Dummy )
	Notch ( 1     0 Dummy )
	) )

	Brake_Hand		( 0 1 1.0 0
		NumNotches	( 0 )
		)

	Brake_Engine	( 0 1 0.07 0.5
		NumNotches	( 1
		Notch		( 0	1 Dummy )
	) )

comment ( Prubezna brzda typ Skoda N/O )
           Brake_Train ( 0 1 0.03 0 
                NumNotches ( 5
                    
		    Notch ( 0.2  0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.3  0 TrainBrakesControllerReleaseStart ) 
                    Notch ( 0.45 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.95 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 1 0 TrainBrakesControllerEmergencyStart )  
                  
                    
                    
                )
            )

	)
	
Comment	( Operations )

	Description (
	"Rada 141 CD je univerzalni elektricka kapotova lokomotiva\n\n"+
	"Max. provozni rychlost:  120km/h TBZ=132km/h\n\n"+
	"Hmotnost plne vyzbroj. lokomotivy: 84tun\n\n"+
	"Vykon 38% odpovida hospodarnemu seriovemu stupni\n\n"+ 
	"Vykon 64% odpovida hospodarnemu serioparalelnimu stupni\n\n"+
	"Vykon hodinovy : 2344kW\n\n"+
	"Vykon trvaly   : 2032kW\n\n"+
	"Tazna sila na haku  : 205kN\n\n"+
	"Proud p?i Ft = 200kN : 550A\n\n"+
	"Proud p?i Ft = 175kN : 500A\n\n"+
	"Proud p?i Ft = 160kN : 450A\n\n"+
	"Pretizeni:\n"+
	"Proud trvaly : 360A\n\n"+
    		"60min: 415A\n\n"+
    		"45min: 455A\n"+
    		"30min: 510A\n"+
    		"15min: 605A\n"+
	"Brzda DAKO-L\n\n"+
	"Brzdic prubezne vlakove brzdy Skoda N/O\n\n"+
	"Brzdic lokomotivni brzdy DAKO-BP\n\n"
    	)

   	EngineOperatingProcedures (
		"Stupne kontroleru:\n"+
		"1.-23.	Rozjezdove stupne seriove\n"+
		"24.	Hospodarny seriovy stupen (odporniky vyrazeny)\n"+
		"I.-IV.	Shuntovaci rozjedove stupne, vsechny motory v serii\n"+
		"A.B.C.	Prechodove stupne serie - > serioparalel\n"+
		"25.-32.Odporove serioparalelni stupne (vzdy dva motory v serii)\n"+
		"33.	Hospodarny serioparalelni stupen (odporniky vyrazeny)\n"+
		"I.-V.	Shuntovaci stupne pro serioparalelni zapojeni motoru\n\n"
	)
	
)
