SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( csd_T4751502
	comment( upravil Ppoollll & Jacek & O.Frinta & Ondra Janiš  - verze 1.0 )
	Comment ( Datum: 05/02/2011 )
	Comment ( Version: 1.01 )
	Comment ( Model: Juraj Prodaj 2010 )
	Comment ( Svetla CSD Tadeus )

	Type ( Engine )
	WagonShape ( csd_T4751502.s )

	Size ( 3m 4.4m 13.33m )
	CentreOfGravity ( 0m 1.9m 0m )
	Mass ( 64.0t )
	WheelRadius ( 50cm )
	InertiaTensor ( Box ( 3m 4.4m 13.33m ) )
	Coupling (
            Type ( Chain )
            Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
            )
		Velocity ( 0.01m/s )
	)
	
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 8cm )
	DerailRailForce ( 2.5*64t )
	DerailBufferForce ( 630kN )
comment( počet náprav )
	NumWheels (	4 )
comment( přepočteno na počet náprav - síly určující jízdní odpory )
	Friction (
		926N/m/s		0		1mph		16.38N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "handbrake, graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 60kN )

	MaxHandbrakeForce( 20kN )
	NumberOfHandbrakeLeverSteps( 100 )

	EmergencyBrakeResMaxPressure( 73 )
	TripleValveRatio( 1.24 )
	MaxReleaseRate( 2 )
	MaxApplicationRate( 2 )
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 10 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 28 )


	IntakePoint ( 0 1.0 FuelDiesel )

Comment (kapacita cestujících - jen kvůli tvorbě JŘ v misích)
	PassengerCapacity ( 110.0 )

Comment	( Lights )

Lights ( 30
	Comment ( Svetla verze CSD by Tadeus )
		Comment ( Svetelne kuzely )
		Light (
		Comment ( Svetelny kuzel tlumeny ( tma ) )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 1.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0 1.52 0 )
				Angle ( 25 )
				Transition ( 1 )
				Radius ( 25 )
		)	)	)
		Light (
		Comment ( Svetelny kuzel plny ( tma ) )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 2.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 1.52 0 )
				Angle ( 15 )
				Transition ( 1 )
				Radius ( 50 )
		)	)	)
		Light (
		Comment ( Svetelny kuzel stredni ( svetlo ) )
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 2.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0 1.52 0 )
				Angle ( 15 )
				Transition ( 1 )
				Radius ( 35 )
		)	)	)
		Comment ( Reflektory )
		Light (
		Comment ( Predni reflektor tlumeny PK )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Headlight ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.0 3.79 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni reflektor plny PK )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Headlight ( 3 )
			)
			FadeIn ( 3.5 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0.0 3.79 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Predni reflektor TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.0 3.79 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni reflektor tlumeny ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Headlight ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.0 3.79 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Light (
		Comment ( Zadni reflektor plny ZK )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Headlight ( 3 )
			)
			FadeIn ( 3.5 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFFF )
				Position ( 0.0 3.79 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 1 )
				Radius ( 0.3 )
		)	)	)
		Comment ( Pozicni svetla )
		Light (
		Comment ( Predni leve bile PK jizda den )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( -0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni leve bile PK jizda noc )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( -0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni leve bile TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni leve bile ZK posun tma )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni leve cervene ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave bile PK posun tma )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave bile PK jizda den )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave bile PK jizda noc )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave bile TR )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave cervene ZK )
			Type ( 0 )
			Conditions (
			Unit ( 4 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Predni prave bile LC )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFF99 )
				Position ( 0.67 1.83 6.11 )
				Azimuth ( 0 0 0 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni leve bile ZK posun tma )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFA4 )
				Position ( -0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni leve bile ZK jizda den )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( -0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni leve bile ZK jizda noc )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( -0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni leve cervene PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni leve cervene TR )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( -0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave bile ZK jizda noc )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Service ( 2 )
			Control ( 2 )
			Headlight ( 4 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave bile ZK jizda den )
			Type ( 0 )
			Conditions (
			Unit ( 5 )
			Service ( 2 )
			Control ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave bile PK posun tma )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFFC4 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave cervene PK )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 2 )
			Service ( 2 )
			Headlight ( 4 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave cervene TR )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFF0000 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
		)	)	)
		Light (
		Comment ( Zadni prave bile LC )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
				Duration ( 0 )
				LightColour ( FFFFFF99 )
				Position ( 0.67 1.83 -6.11 )
				Azimuth ( 180 180 180 )
				Transition ( 0 )
				Radius ( 0.2 )
	)	)	)	)
    	Sound (   "../../common.snd/snddlok/742eng.sms"  )
)

Engine ( csd_T4751502
	Effects (
		DieselSpecialEffects (
			Exhaust1 (
					0.0 4.6 -1.2
					0 1 0
					0.1
			)
		)
	)
	Wagon ( csd_T4751502 )
	Type ( Diesel )
	MaxPower ( 780kW )
	MaxForce ( 192kN )
	MaxContinuousForce ( 121kN )
	MaxVelocity ( 90km/h )
	MaxCurrent ( 590A ) 
	WheelRadius ( 0.5m )
	Sanding ( 15km/h )
	NumWheels ( 4 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

	AirBrakesAirCompressorPowerRating( 2.55 )
	AirBrakesMainMinResAirPressure( 56 )
	AirBrakesMainMaxAirPressure( 144 )
	AirBrakesMainResVolume( 35 )
	AirBrakesAirCompressorWattage( 35kW )
	AirBrakesCompressorRestartPressure( 121 )

	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.5 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.81 )
	EngineBrakesControllerMaxApplicationRate( 10 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerEmergencyApplicationRate( 15.0 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 59 )
	comment(EngineBrakesControllerMinPressureReduction( 5 ))
	comment(EngineBrakesControllerMaxPressureDropInNormalApplication ( 22.5 ))
	Comment( EngineBrakesControllerFullServicePressureDrop( 22.5 ))
	
	TrainBrakesControllerMinPressureReduction( 3 )	
	TrainBrakesControllerMaxApplicationRate( 2 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate ( 4.0 )
	TrainBrakesControllerEmergencyApplicationRate( 15.0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxPressureDropInNormalApplication ( 22.5 )
	TrainBrakesControllerMaxSystemPressure( 73 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 22.5 )
	TrainPipeLeakRate( 0.1 )
		
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Independent, Train" )

	EngineBrakesControllerDirectControlExponent( 1 )

      CabView ( "..//..//common.cab//cab742//742.cvf"  )
	HeadOut ( 1.8 3.0 -3.4 )

 	MaxDieselLevel ( 4000l )
	DieselUsedPerHourAtMaxPower ( 245l )
	DieselUsedPerHourAtIdle ( 9l )

	DieselSmokeEffectInitialMagnitude( 1.0 )
	DieselSmokeEffectMaxMagnitude( 2.0 )

	DieselSmokeEffectInitialSmokeRate( 0.5 )
	DieselSmokeEffectMaxSmokeRate( 2.5 )

	DieselEngineIdleRPM( 510 )
	DieselEngineMaxRPM( 1250 )
	DieselEngineSpeedOfMaxTractiveEffort( 19.6km/h )
      DieselEngineMaxRPMChangeRate( 100 )

	DoesHornTriggerBell( 0 )

	MaxSandingTime( 2000 )
	comment( 320kg )

	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 1 )
    		)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)
		
	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 20 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 90 )
		MonitoringDeviceCriticalLevel( 65 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed( 5 )
		MonitoringDeviceDoesSuppressionReset( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 4 )
		MonitoringDeviceTriggerOnOverspeed( 64 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
	EngineVariables( 4000 )
			
        EngineControllers (
            Throttle ( 0 1 0.04 0
                NumNotches ( 9
                    Notch ( 0       0 Dummy )
                    Notch ( 0.038   0 Dummy )
                    Notch ( 0.090   0 Dummy )
                    Notch ( 0.167   0 Dummy )
                    Notch ( 0.308   0 Dummy )
                    Notch ( 0.449   0 Dummy )
                    Notch ( 0.641   0 Dummy )
                    Notch ( 0.821   0 Dummy )
                    Notch ( 1       0 Dummy )
                )
            )
            Brake_Engine ( 0 1 0.125 1
                NumNotches( 1
                    Notch(0    1 Dummy )
                )
            )            
            comment(***Prubezna brzda typ DAKO-BS2***)            
           	Brake_Train ( 0 1 0.020 0.14
                NumNotches ( 7
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
			  Notch ( 0.14 0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.21 0 TrainBrakesControllerNeutralhandleOffStart )
			  Notch ( 0.33 0 TrainBrakesControllerMinimalReductionStart )
                    Notch ( 0.35 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.87 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 1.00 0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
		     NumNotches( 1
                    Notch(0    1 Dummy)
                )
            )
            DirControl ( -1 0 1 1 )
		AWS ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
		Vigilance ( 0 1 0 )
            Wipers ( 0 1 0 )
            comment (EmergencyStopResetToggle( 0 1 0 ))
            EmergencyStopToggle( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
        )
        
    	Name ("CSD T475.1502")
    	Description (
		"Rada 744 CD je univerzálni dieselelektrická kapotovaná lokomotiva pro pouzití od posunovacího provozu pres tazení osobních vlaku az do tazení stredne tezkých nákladních vlaku v dvojclenném rízení.\n\n"+
		"Usporádání dvojkolí: Bo'Bo'\n\n"+
		"Prenos výkonu: elektrický\n\n"+
		"Zdroj výkonu: naftový motor CKD K 6 S 230 DR\n\n"+
		"Výkon: 883kW\n\n"+
		"Max. provozní rychlost:  90km/h\n\n"+
      	"Max. tazná síla na háku: 192kN\n\n"+
		"Trvalá tazná síla na háku: 121kN\n\n"+
		"Max. výska: 4722mm\n\n"+
		"Délka pres nár.: 13600mm\n\n"+
		"Max. sírka: 3060mm\n\n"+
		"Hmotnost se 2/3 vyzbroj. lokomotivy: 64t"  
    	)
    	EngineOperatingProcedures (
		"Jak se rozjet:\n"+
		"1.	Stisknete W na prestavení reverzního kontoleru do polohy 'vpred'.\n"+
		"2.	Stisknete a drzte ; pro odbrzdení vlakové brzdy.\n"+
		"(3.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy.)\n"+
		"4.	Stisknete D pro zvýsení pozadovaného výkonu.\n"+
		"5.	Pomalu zvysujte výkon stiskem D, dokud vlak nedosáhne pozadované rychlosti.\n"+
		"6.	Jakmile se vlak rozjede tak jedním stiskem ' presunte vlakovou brzdu do polohy ZÁVER.\n\n"+
		"Jak zpomalit\n"+
		"1.	Stisknete A pro snízení pozadovaného výkonu (postupne az na 0).\n"+
		"2.	Jestlize je to nutné tak pouzijte brzdy pro postupné rychlejsí snizování rychlosti.\n\n"+
		"Jak pouzít vlakovou brzdu\n"+
		"1.	Stisknete a drzte ' nez presunete rukojet brzdy do polohy brzdeni a dosáhnete pozadovaného brzdného tlaku.\n"+
		"2.	Po dosazení pozadovaného brzdného tlaku stiskem ; presunte rukojet brzdy do polhy ZÁVER.\n\n"+
		"Jak odbrzdit vlakovou brzdu\n"+
		"1.	Stisknete a drzte ; az presunete rukojet brzdy do polohy PLNENÍ.\n"+
		"2.	Pockejte, az klesne tlak v brzdových valcích na 0.\n"+
		"3.	Po odbrzdení a uvedení vlaku do pohybu stisknete ' pro presunutí rukojeti brzdy do polohy ZÁVER.\n\n"+
 		"Jak pouzít lokomotvní brzdu\n"+
		"1.	Stisknete a drzte ] pro zabrzdení lokomotivní brzdy (0-100%).\n\n"+
		"Jak odbrzdit lokomotivní brzdu\n"+
		"1.	Stisknete a drzte [ pro odbrzdení lokomotivní brzdy (0%).\n\n"+
		"Jak pouzít záchrannou brzdu\n"+
		"1.	Stisknete a drzte A pro snízení výkonu az na 0.\n"+
		"2.	Stisknete BACKSPACE pro aktivaci záchrané brzdy.\n\n"+
		"Jak zrusit záchrannou brzdu\n"+
		"1.	Pockejte na úplné zastavení vlaku.\n"+
		"2.	Stisknete Z pro odblokování ovládání lokomotivy.\n"+
		"3.	Stisknete ; a [ pro odbrzdení brzdných systému.\n"+
		"4.	Pomalu zvysujte výkon stiskem D .\n\n"+
		"Jak zmenit smer\n"+
		"1.	Zastavte vlak.\n"+
		"2.	Presunte paku reverzniho kontroleru do polohy vzad nebo vpred dvojitým stiskem S.\n"+
		"3.	Odbrzdete brzdy stiskem ; (prípadne [ ).\n"+
		"4.	Pomalu zvysujte vykon stiskem D .\n\n"+
  		"Výstup a nástup cestujících\n"+
		"1.	Zastavte ve stanici.\n"+
		"2.	Stisknete ENTER pro zahájení výstupu a nástupu cestujících.\n"+
		"3.	Pockejte na signál k odjezdu.\n"+
		"TIP: Pro zobrazení casu príjezdu a odjezdu u této a následující stanice pouzijte klávesu F10.\n\n"+
		"Jak pripojit vagony/lokomotivy:\n"+
		"1.	Najedte pomalu na soupravu (optimální rychlost 1 km/h).\n"+
		"Tip: Pro zobrazení pohledu na spráhlo stisknete klávesu 6.\n"+
		"2.	Stisknete F9 pro otevrení okna se seznamem lokomotiv a vagonu ve vlaku.\n"+
		"3.	Jestlize je ikona vozu cervená, je zatazena rucní brzda. Dvojtukem mysí na voze uvolníte/zatáhne rucní brzdu.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9.\n"+
		"5.	Pockejte az odbrzdíte pripojené vozy.\n\n"+
		"Odpojení vozu nebo lokomotivy\n"+
		"POZOR! Melo by se provádet jen tehdy, pokud VLAK STOJÍ!\n"
		"1.	Otevrete okno sestavy vlaku F9.\n"+
		"2.	Poklepejte 2x na ikonu vozu, ktery se má odpojit, pokud chcete, aby mel vuz zatazenou rucní brzdu.\n"+
		"3.	Poklepejte mysi 2x na ikonu spoje, kde ma byt vlak rozdelen.\n"+
		"4.	Zavrete okno sestavení vlaku stiskem F9."
		"Jak doplnit naftu\n"+
		"1.	Zastavte u naftového stojanu stredem nádrze.\n"+
		"2.	Stisknete klávesu T a drzte ji po dobu doplnování nafty stisknutou.\n"+
		"TIP: Pro zobrazení prubehu plnení nádrze stisknete F9 a klepnete mysí na ikonu lokomotivy.\n\n"+
	)
	Sound (   "../../common.snd/snddlok/742cab.sms"  )
)
